You are using Internet Explorer and will not be able to use our website properly.
Please change to an up-to-date browser for ideal presentation of the website.

x

# Allfit Steel Formwork

Robust steel-framed panel based formwork with Birch Plywood, easy interconnections, and quick assembly for durable and efficient construction.

## Durable Formwork for Demanding Projects

Allfit Steel Formwork is designed to handle the toughest construction challenges, offering unmatched durability and precision while ensuring ease of use for professionals.

- Withstands 60kN/m² Concrete Pressure: Robust panels that meet the highest performance standards.
- Strong Steel Frames: Made from 5mm thick FE350-grade steel, weighing 33.0kg per sq. m. for 3000x900 mm panels, meets deflection limits as per IS codes.
- Innovative Slot Arrangement: Ensures easy configuration, boosting efficiency and accuracy in construction projects.

3D Representation of Allfit Steel Formwork System

## Galvanized and Powder-Coated Panels

With advanced corrosion resistance and superior durability, Allfit Quickfit panels offer reliability across diverse construction environments, ensuring longevity and cost-efficiency.

- Galvanized & Powder-Coated: Protects against corrosion and wear, ensuring long-lasting durability.
- Phenolic-Coated Birch Plywood: 12mm plywood with 120gsm coating for smooth finishes and multiple reuses.
- Custom Sizes Available: Heights from 3.0m to 1.2m and widths from 900mm to 300mm for versatile applications.

3D Representation of how the Allfit Clamp is used to join panels in Allfit System
Allmarc's formwork panels are precisely manufactured using state-of-the-art machining tools, with in-house Robologic and ABB robotic welding arms ensuring accurate welding of the panel components.

## Advantages of Allfit Steel Formwork System

Allfit Steel Formwork offers unmatched strength, durability, and versatility for various construction needs.

- #### Unyielding Steel Frames for Durability

  - High-Strength Steel: 5mm thick FE350 grade.
  - Durability: Withstands up to 60 kN/m² concrete pressure.
  - Deflection Compliance: Meets IS CODES standards.

- #### Birch Plywood with Phenolic Magic

  - Superior Finish: 12mm Birch Plywood with 120gsm phenolic coating.
  - Low Moisture Intake: 15% for enhanced longevity.
  - High Reusability: Suitable for multiple uses.

- #### Galvanized and Powder-Coated Panels

  - Corrosion Resistance: Galvanized and powder-coated finish.
  - Durability: Withstands wear and fading.
  - Cost-Effective: Reliable for diverse projects.

- #### The Unique Slot Arrangement

  - Efficient Configuration: Sturdy and precise panel setups.
  - Innovative Design: Simplifies the formwork process.
  - Enhanced Accuracy: Ensures project efficiency.

- #### Allfit’s Customizable Size Range

  - Height Options: 3.0m, 2.7m, 1.8m, 1.5m, 1.2m.
  - Width Options: 900mm, 750mm, 600mm, 450mm, 300mm.
  - Custom Solutions: Suits various concrete shapes and sizes.

- #### Advanced Protection and Longevity

  - Protection: Against corrosion and wear.
  - Extended Lifespan: Withstands harsh conditions.
  - Maintenance: Low upkeep required.

3D Walkthrough of Allfit Formwork System highlighting how Accessories are used in Assembly

## Essential Accessories for Allfit Steel Formwork System

Explore key accessories designed to enhance the Allfit Steel Formwork System’s performance. These components ensure secure connections, precise alignment, and robust support for efficient formwork setup.

- Allfit Clamp: Connects two panels securely; options available based on project requirements and ease of use at the job site.

- Allfit Adjustable Clamp: Connects fillers with an adjustable range from 0 to 100mm; offers flexibility for various project needs.

- Allfit Filler Waling: Provides stiffening, aligning, and force-transmitting support at panel connections; enhances overall stability.

- Allfit Corner Connector: Joins panels at corners to ensure precise 90° angles; ideal for accurate formwork configurations.

Designed for versatility, they simplify the setup and adjustment of formwork structures.

3D Representation of Accessories in Allform System Assembly
Actual images of our formwork panels showcased at the Constro International Exhibition in Pune.

## Available Sizes of Allfit Steel Formwork Panels

Engineered for versatility and durability, our Allfit Steel Formwork Panels come in a range of widths and heights, designed to meet the demands of various construction projects. Each panel ensures optimal strength, precision, and ease of assembly, making it the ideal choice for forming robust concrete structures.

Sr. No. | Model | Product Name | Width (mm) | Height (mm)
--- | --- | --- | --- | ---
Sr. No. | Model | Product Name | Width (mm) | Height (mm)
1 | AFI3090P/G | Allfit Panel 3000x900 | 900 | 3000
2 | AFI3075P/G | Allfit Panel 3000x750 | 750 | 3000
3 | AFI3060P/G | Allfit Panel 3000x600 | 600 | 3000
4 | AFI3045P/G | Allfit Panel 3000x450 | 450 | 3000
5 | AFI3030P/G | Allfit Panel 3000x300 | 300 | 3000
6 | AFI2790P/G | Allfit Panel 2700x900 | 900 | 2700
7 | AFI2775P/G | Allfit Panel 2700x750 | 750 | 2700
8 | AFI2760P/G | Allfit Panel 2700x600 | 600 | 2700
9 | AFI2745P/G | Allfit Panel 2700x450 | 450 | 2700
10 | AFI2730P/G | Allfit Panel 2700x300 | 300 | 2700
11 | AFI1890P/G | Allfit Panel 1800x900 | 900 | 1800
12 | AFI1875P/G | Allfit Panel 1800x750 | 750 | 1800
13 | AFI1860P/G | Allfit Panel 1800x600 | 600 | 1800
14 | AFI1845P/G | Allfit Panel 1800x450 | 450 | 1800
15 | AFI1830P/G | Allfit Panel 1800x300 | 300 | 1800
16 | AFI1590P/G | Allfit Panel 1500x900 | 900 | 1500
17 | AFI1575P/G | Allfit Panel 1500x750 | 750 | 1500
18 | AFI1560P/G | Allfit Panel 1500x600 | 600 | 1500
19 | AFI1545P/G | Allfit Panel 1500x450 | 450 | 1500
20 | AFI1530P/G | Allfit Panel 1500x300 | 300 | 1500

## Looking for Customised Solutionsfor your Project?

Allmarc team will be happy to help you find the ideal solutions tailored to your business or project requirement.
Submit Inquiry Call our Specialist
Inquiry
Whatsapp
Call
Send Inquiry for
Get assured response within 24 hours.

Full name
Company name
Phone
Email ID
Your Message
Your message has been sent successfully!