You are using Internet Explorer and will not be able to use our website properly.
Please change to an up-to-date browser for ideal presentation of the website.

x

# Formwork Beams

Allmarc offers a range of beams tailored for formwork support, including Primary Beams, Steel Timber Secondary Beams, and lightweight Allbeam options in both single and double webbed aluminum designs. Our beams ensure high load capacity and precise performance, with the Allslim Soldering Beam providing added strength for versatile construction needs.

### Noise Barrier

For producing noise barriers used in high-speed rail, highways, and urban infrastructure.

### U Cable Duct Moulds

Designed to create U-shaped cable ducts for housing and protecting underground cables.

### Track Slab Moulds

Used in the construction of track slabs for railways, providing a stable and durable base.

## Primary Beam

The Primary Beam is an essential component for slab formwork, ensuring superior support and stability. With its unique triangular perforations for efficiency and a reinforced wooden insert, it provides durability and precision for various formwork applications.

- Triangular Perforations: Reduces overall weight while maintaining structural strength and stability.
- Reinforced Wooden Insert: Enhances load-bearing capacity and ensures long-lasting durability in demanding conditions.
- Versatile Application: Suitable for slab formwork and shoring, adaptable to a wide range of construction needs.

3D Representation of Slab Formwork involving Primary Beams, Secondary Steel Timber Beam and Birch Ply

## Advantages of Primary Beam

Allmarc’s Primary Beam offers superior load support, precision, and stability in slab formwork. Its lightweight design and high flexural rigidity ensure efficient handling and accurate slab casting, making it an essential choice for robust construction projects.

- #### Heavy-Duty Load Support

  - With a moment (M) of 5 kN.m, the Primary Beam is tailored for heavy load-bearing, making it indispensable in supporting elevated slabs during construction.

- #### Optimal Flexural Rigidity

  - Boasting a flexural rigidity (EI) of 210 kNm², it resists deformation under load, ensuring the precision and stability required in slab formwork and shoring applications.

- #### Efficient Weight Distribution

  - Weighing 3 kg/m, the beam strikes a balance between strength and maneuverability, facilitating ease of handling and installation in formwork and shoring setups.

3D Walkthrough of Allmarc's Primary Beam

## Specification of Primary Beam

Allmarc's Primary Beam is engineered for optimal performance in slab formwork, ensuring exceptional support and stability.

- Sizes: Available in 1.8m, 2.4m, and 3m lengths
- Moment (M): Capable of withstanding 5 kN·m
- Shear Force (Fs): Designed for a maximum shear force of 8 kN
- Flexural Rigidity (EI): 420 kN·m² for enhanced structural integrity
- Weight: Lightweight at 7.52 kg/m for ease of handling
- Section Dimensions: 150 mm (H) x 80 mm (W), optimized for strength and stability

## Looking for Customised Solutionsfor your Project?

Allmarc team will be happy to help you find the ideal solutions tailored to your business or project requirement.
Submit Inquiry Call our Specialist
Inquiry
Whatsapp
Call
Send Inquiry for
Get assured response within 24 hours.

Full name
Company name
Phone
Email ID
Your Message
Your message has been sent successfully!