You are using Internet Explorer and will not be able to use our website properly.
Please change to an up-to-date browser for ideal presentation of the website.

x

# Allstage Staging System

Robust, 8 MT load capacity for heavyweight construction, upto 48 mm pipe diameter for stability, and a streamlined spring locking system for efficient, safe assembly.

## Overview of Allstage Staging System

The Allstage Staging System by Allmarc is a high-performance, adaptable solution for construction projects requiring quick and efficient staging. Built with precision and engineered for durability, it ensures fast assembly, minimal components, and exceptional load-bearing capacity, making it ideal for both small and large-scale scaffolding needs.

- Quick assembly with fewer components.
- High-grade steel construction for enhanced durability.
- Excellent load-bearing capacity for heavy-duty applications.
- Adaptable design for various project layouts.
- Lightweight for easy handling and transport.
- Ideal for both construction and maintenance work.

3D Representation of Allstage Staging System

## Key Features of Allstage Staging System

The Allstage Staging System is designed for efficiency, flexibility, and safety in various construction and industrial projects.

- #### Quick Assembly

  - Minimal components enable fast installation and dismantling.
  - Reduces downtime, improving project efficiency.

- #### Versatile Design

  - Adapts to complex structures, ensuring support in challenging areas.
  - Ideal for both simple and intricate layouts.

- #### Durable Construction

  - Manufactured with high-grade steel for long-term durability.
  - Withstands harsh environmental conditions.

- #### Stable Connections

  - Secure joint fastening for enhanced stability and safety.
  - Prevents slippage and misalignment during operations.

- #### Lightweight Structure

  - Easy to handle and transport while maintaining strength.
  - Reduces labor intensity and transportation costs.

- #### Customizable Heights

  - Adjustable vertical and horizontal members cater to varied project needs.
  - Offers flexibility in height configuration for different applications.

3D walkthrough of how Verticals, Ledgers and Braces are attached with each other.

## Verticals for Allstage Staging System

The Verticals in the Allstage Staging System are essential load-bearing members, designed for high strength and durability. They are crafted from top-grade YST 310 steel and feature precision-engineered components for maximum efficiency in heavy-duty applications.

- Steel Type:

  - YST 310 Steel (60% stronger than YST 210)
  - Higher load-bearing capacity for demanding projects

- Rosset Plates:

  - Welded at 500 mm intervals
  - Laser-cut for precision
  - Robotic welding ensures consistency and dimensional accuracy

- Sectional Properties:

  - Diameter: 48.3 mm
  - Thickness: 3.2 mm
  - Sectional Area: 4.53 cm²
  - Moment of Inertia: 11.59 cm⁴
  - Section Modulus: 4.8 cm³

Actual Images of Verticals for Allstage Staging System at Allmarc Factory
3D walkthrough of Verticals in Allstage Staging System

## Specification of Verticals for Allstage Staging System

Our vertical components are designed with precision to support diverse construction needs while ensuring safety and efficiency on-site.

Part Code | Component | Pipe Dia. x Thick, mm | Length, mm | No. of Rings
--- | --- | --- | --- | ---
ATV-1000 | Vertical | 48.3 x 3.2 | 1000 | 2
ATV-1500 | Vertical | 48.3 x 3.2 | 1500 | 3
ATV-2000 | Vertical | 48.3 x 3.2 | 2000 | 4
ATV-2500 | Vertical | 48.3 x 3.2 | 2500 | 5
ATV-3000 | Vertical | 48.3 x 3.2 | 3000 | 6

## Ledgers for Allstage Staging System

Ledgers are vital horizontal components in shoring systems, designed to support horizontal and lateral loads from planks and walkways. With crimped pipes, investment-cast end connectors, and secure attachment via Rosset plates, Ledgers feature a built-in locking mechanism for stable diagonal bracing.

- Material Properties

  - Steel Grade: YST 310 (60% stronger than YST 210)

- Sectional Properties

  - Sectional Area: 4.53 cm²
  - Moment of Inertia: 11.59 cm⁴
  - Section Modulus: 4.8 cm³
  - Diameter: 48.3 mm
  - Thickness: 3.2 mm

- Design Features

  - End Connectors: Investment casted for maximum strength
  - Rosset Plate Connection: Ensures secure attachment to vertical members
  - Locking Mechanism: Facilitates secure bracing connections

Actual Images of Ledgers for Allstage Staging System at Allmarc Factory
3D Walkthrough of Ledger in Allstage Staging System

## Specification of Ledgers for Allstage Staging System

Our ledger components are meticulously engineered to support various construction applications while ensuring safety and efficiency on-site.

Part Code | Component | Pipe Dia. x Thick, mm | Length, mm | Point Load, (W), kN | Two Point Loads, (P+P), kN | Total Load, kN (UDL, kN/m)
--- | --- | --- | --- | --- | --- | ---
ATL-1200 | Ledger | 48.3 x 3.2 | 1200 | 1.95 | 2.50 | 3.42 (2.85)
ATL-1500 | Ledger | 48.3 x 3.2 | 1500 | 1.38 | 1.62 | 2.21 (1.47)
ATL-1800 | Ledger | 48.3 x 3.2 | 1800 | 0.97 | 1.13 | 1.53 (0.85)
ATL-2400 | Ledger | 48.3 x 3.2 | 2400 | 0.71 | 0.87 | 1.13 (0.47)
ATL-3000 | Ledger | 48.3 x 3.2 | 3000 | 0.57 | 0.69 | 0.90 (0.30)

## Braces for Allstage Staging System

Bracings are diagonal members in the shoring system designed to take inclined loads, transmitting forces directly along their axes. They ensure maximum structural stability and safety in various construction applications.

- Material Properties:

  - Steel Grade: YST 310 (approximately 60% stronger than YST 210)

- Locking Mechanism:

  - Bracings are pressed into the slots in the ledgers for enhanced strength. A pin is then inserted to lock them securely in place.

- Sectional Properties:

  - Diameter: 42.4 mm
  - Thickness: 3.2 mm
  - Sectional Area: 3.94 cm²
  - Moment of Inertia: 7.61 cm⁴
  - Section Modulus: 3.58 cm³

Actual images of Braces for Allstage Staging System at Allmarc Factory
3D Walkthrough of Braces for Allstage Stagin System

## Specification of Braces for Allstage Staging System

Our bracing components are meticulously engineered to support various construction applications while ensuring safety and efficiency on-site.

Part Code | Component | Pipe Dia. x Thick, mm | Length, mm
--- | --- | --- | ---
ATB-1200 | Bracing | 48.3 x 3.2 | 1000
ATB-1500 | Bracing | 48.3 x 3.2 | 1500
ATB-1800 | Bracing | 48.3 x 3.2 | 2000
ATB-2400 | Bracing | 48.3 x 3.2 | 2500

## Looking for Customised Solutionsfor your Project?

Allmarc team will be happy to help you find the ideal solutions tailored to your business or project requirement.
Submit Inquiry Call our Specialist
Inquiry
Whatsapp
Call
Send Inquiry for
Get assured response within 24 hours.

Full name
Company name
Phone
Email ID
Your Message
Your message has been sent successfully!