You are using Internet Explorer and will not be able to use our website properly.
Please change to an up-to-date browser for ideal presentation of the website.

# Specialty Formwork Solutions by Allmarc

Allmarc offers cutting-edge specialty formwork solutions tailored to the unique needs of construction projects. Our innovative designs prioritize durability, efficiency, and precision, making us a trusted partner in complex infrastructure developments.

### Allwell Deep Foundation

Enhances large-diameter excavations with corrugated steel liner plates and precise grouting for superior soil stabilization.

### Seismic Stopper

Provides support to protect structures from seismic impacts, ensuring stability and safety. Fixed and Movable Seismic Stoppers available.

# Allwell Deep Foundation

Allmarc’s Allwell Deep Foundation excels in large-diameter excavations, using corrugated steel liner plates and meticulous grouting for enhanced soil stabilization. Ideal for urban and railway-adjacent projects, it ensures robust support and minimal disruption.

## Advanced Solution for Large-diameter Excavations

The Allwell Deep Foundation is an advanced solution designed to handle large-diameter excavations ranging from 6 to 11 meters. This system utilizes circular corrugated steel liner plates and precise grouting to offer exceptional soil stabilization and support.

- Large-Diameter Excavation Support: Engineered to manage large diameters from 6 to 11 meters, using robust steel liner plates to support the bore wall.
- Superior Soil Stabilization: Meticulous grouting between the liner plates and surrounding soil enhances soil stabilization and reinforcement.
- Precision Engineering: Equipped with a top guide frame for accurate alignment and positioning of the formwork.
- Enhanced Practicality: Features a ladder for easy worker access, a collapsible roof for weather protection, and a reinforcement fixing jig for efficient cage lowering.

Perfect for urban areas and railway-adjacent projects, the Allwell Deep Foundation ensures minimal disruption while protecting railway foundations from vibrations and structural issues.

Pier Moulds made for MAHSR Project.
Allmarc was honoured to host the stakeholders of NHSRCL - TCAP - DRA at our factory premises to examine the very revolutionary ALLWELL Deep Foundation System.

## Manufacturing Process for Allwell Deep Foundation

Our manufacturing process for Allwell Deep Foundation ensures precision and quality through a series of advanced steps, from raw material handling to final assembly.

- Raw Material Inward: Sheets in coil form are received and inspected via Material Inspection Report (MIR).
- Forming: Sheets are shaped using a specialized roll forming machine.
- Hole Punching: Holes are precisely punched into the formed sheets.
- Curving: Sheets are curved to diameters ranging from 6 to 11 meters.
- Gauging: Sensors are used to ensure accurate measurements and alignment.
- Cutting: Automated hydraulic shear press cuts the sheets to required sizes.
- Liner Sheet and Curve Beam Formation: End plates and curve beams are formed to create the final shape.
- End Plate Welding: Robotic welding ensures precise and strong end plate attachments.

Visual glimpse of the manufacturing process of Allwell Deep Foundation.

# Seismic Stopper

Allmarc's Seismic Stoppers safeguard structures from seismic damage by absorbing and restraining seismic forces. Available in fixed and movable designs, they ensure stability and safety during earthquakes with their high-quality materials and precise engineering.

## Fixed Seismic Stopper

Allmarc's Fixed Seismic Stopper is a critical component designed to safeguard structures from seismic forces, ensuring structural integrity during earthquakes. This reliable device acts as a restraint to mitigate seismic impacts, offering consistent protection and enhanced safety for buildings. Key benefits:

- Seismic Protection: Effectively restrains seismic forces to prevent structural damage.
- Enhanced Structural Safety: Contributes to the overall stability and safety of buildings.
- Efficient and Reliable: Delivers consistent performance in mitigating seismic impacts.
- Non-Invasive Design: Easily integrated into existing structures without significant modifications.

### Specifications:

- Height: 300mm x 300mm x 1760mm
- MS Plate (Stopper): E350 B0 as per IS 2062
- Rubber: Chloroprene & Sponge as per specification & material criteria
- I Bolt: 8.8 Grade as per IS 4190

3D Representation of Fixed Seismic Stopper.
Allmarc's Seismic Stoppers were supplied to MAHSR Project. Here's a 3D representation of where those stoppers are used.

## Movable Seismic Stopper

The Movable Seismic Stopper offers versatile protection against seismic impacts with its high-quality components and flexible design. This innovative solution provides dynamic seismic resilience, allowing for easy movement and deployment to safeguard structures during earthquakes. Key benefits:

- Seismic Resilience: Enhances stability and protects structures from earthquake impacts.
- Mobility and Versatility: Allows for flexible placement and adaptation to various construction needs.
- High-Quality Components: Ensures reliable performance with durable materials.
- Enhanced Structural Safety: Contributes to overall structural integrity and safety.

### Specifications:

- Height: 300mm x 300mm x 1455mm
- MS Plate (Stopper): E350 B0 as per IS 2062
- MS Plate (Top Cover): E250 B0 as per IS 2062
- Rubber: Chloroprene as per specification & material criteria
- I Bolt: 8.8 Grade as per IS 4190
- Screw Stock Nut: 8.8 Grade as per IS 1363

3D Representation of Movable Seismic Stopper.
Inquiry
Whatsapp
Call
Send Inquiry for
Get assured response within 24 hours.

Full name
Company name
Phone
Email ID
Your Message
Your message has been sent successfully!