You are using Internet Explorer and will not be able to use our website properly.
Please change to an up-to-date browser for ideal presentation of the website.

x

# Cuplock System

Quick assembly, adaptability in confined spaces, and a robust 8 MT loading capacity for strength and durability.

## Heavy-duty Cuplock System

Lightweight, robust, and designed for quick assembly, our Cuplock system delivers reliable fastening and enhanced safety, making it ideal for a range of applications from construction to demolition. Standard specifications for quick reference:

- Outer Diameter: 60 mm
- Thickness: 3.2 mm
- Sectional Area: 4.53 cm²
- Moment of Inertia: ~25.19 cm⁴
- Section Modulus: 8.15 cm³
- Material Grade: YST 310 Steel (60% stronger than YST 210, higher load capacity)
- Hollow Pipe Jack Length: 230 mm, 350 mm, 450 mm, 600 mm
- MS Solid Jack Length: 300 mm, 350 mm, 450 mm, 600 mm

3D Representation of Allmarc Cuplock System
3D walkthrough of locking mechanism in Cuplock System

## Key Components of Cuplock System

Allmarc’s Cuplock System delivers robust, flexible, and secure scaffolding solutions for complex construction needs.

- #### Cuplock Standards or Verticals

  - Made from 60 mm OD MS round pipes.
  - Cup joints welded at 500 mm intervals (customizable).
  - Top cups made from malleable casting for durability.

- #### Cuplock Ledger or Horizontal

  - Forged ledger blades for seamless connection with verticals.
  - 48 mm OD MS round pipes with 3 mm thickness.
  - Customizable as per client requirements.

- #### U-Head Jack

  - Allows for additional height adjustment on vertical standards.
  - Adjustable length: 300 – 600 mm.
  - Supports up to 4 tons load capacity.

- #### Base Jack

  - Ensures stability at the bottom of verticals for uneven ground.
  - Load-bearing capacity of up to 4 tons.
  - Constructed with 48 mm OD hollow pipe and 38 mm OD solid rod.

- #### Top Cup

  - Forged top cup for extended lifespan, surpassing market standards.
  - Movable, sliding along vertical standards for versatile application.
  - Secures ledger, ensuring scaffolding stability and integrity.

- #### Bottom Cup

  - Fixed to the vertical standard for reliable support.
  - Supports ledger for uniform load distribution.

Actual images of Allmarc's cuplock system

## Looking for Customised Solutionsfor your Project?

Allmarc team will be happy to help you find the ideal solutions tailored to your business or project requirement.
Submit Inquiry Call our Specialist
Inquiry
Whatsapp
Call
Send Inquiry for
Get assured response within 24 hours.

Full name
Company name
Phone
Email ID
Your Message
Your message has been sent successfully!