You are using Internet Explorer and will not be able to use our website properly.
Please change to an up-to-date browser for ideal presentation of the website.

x

# Grip Strut

Allmarc’s grip strut anti-skid decking are lightweight, durable, and designed for maximum safety, providing optimal support for modular scaffolding systems worldwide.

## Grip Strut - India's Leading Anti-Slip Solution

Grip Strut by Allmarc is engineered to deliver an ultra-safe, slip-resistant walking surface ideal for challenging environments affected by mud, ice, or oil. Its serrated surface and diamond-shaped openings ensure superior grip and effective debris management, making it an essential solution for enhanced safety and efficiency across industries.

- Offers exceptional slip-resistance for hazardous environments.
- Quick and easy installation with lightweight, durable planks.
- Self-cleaning surface that drains mud, fluids, and debris.
- Suitable for diverse working and walking conditions.

3D Representation of Allmarc Planks
3D walkthrough of locking mechanism in Cuplock System

## R13 slip grade with a slip angle up to 46°

The Anti-Skid Ramp Test conducted by Anulabs in Delhi tested Grip Strut under both dry and wet load conditions, demonstrating its superior slip resistance. With an impressive slip angle of 46 degrees, Grip Strut achieved an Anti-Slip Grade of R13, underscoring its ability to provide excellent traction in hazardous conditions.

- Achieved Anti-Slip Grade of R13 in both dry and wet load oil tests.
- Tested slip angle reached 46 degrees, highlighting its exceptional slip resistance.
- Provides superior traction in challenging conditions, enhancing worker safety.

3D Representation of Allmarc Planks
Actual Image of Allmarc's Allforte Forged Corner Connecter and Roll-formed Profile

## Key Features of Grip Strut

Grip Strut by Allmarc delivers unparalleled safety, strength, and versatility for demanding environments.

- #### Certified R13 Slip Rating

  - Industry-leading R13 slip rating for top-tier safety of workers.
  - Slip angle of up to 46° ensures superior grip on slick surfaces.

- #### Lightweight and Strong

  - 40% lighter than traditional bar gratings.
  - High strength-to-weight ratio allows longer spans and added structural integrity.

- #### Quick & Easy Installation

  - Simple installation using bolts, clamps, or welding for fast deployment.
  - Reduces labor costs and installation time.

- #### Robust Durability

  - Long lifespan with minimal wear, reducing maintenance needs.
  - Built to withstand harsh industrial conditions.

- #### Hot-Dip Galvanized Coating

  - Enhanced corrosion protection with long-lasting hot-dip galvanization.
  - Suitable for outdoor and harsh industrial environments.

- #### Multi-Directional Grip

  - Serrated surface ensures grip in all directions, preventing slips and falls.
  - Excellent for environments with oil, mud, or snow hazards.

- #### Monolithic One-Piece Design

  - Manufactured without joints or welds for added strength and durability.
  - Reduces weak points, enhancing safety and longevity.

- #### Heavy-Duty Options

  - Available in thicker versions for more demanding applications.
  - Extra strength and durability for heavy-load environments.

- #### Customizable Sizing

  - Available in various sizes to meet specific project needs.
  - Adaptable to a wide range of applications in different industries.

## India’s Exclusive Manufacturer of Grip Strut

Allmarc is India’s sole manufacturer of Grip Strut walkways, platforms, and gratings, delivering unmatched quality and safety standards. With state-of-the-art facilities, Allmarc ensures reliable and timely production for any project size.

- Exclusively manufacturing Grip Strut in India.
- High-quality production meeting international safety standards.
- Trusted by industries nationwide for durable, safe platforms.

3D Representation of Allmarc Planks
Actual images of our planks at Allmarc factory

## Grip Strut Fixing Accessories for Fast Installation

Grip Strut units ensure fast and efficient installation with easy attachment to any support structure using standard Diamond Anchors or specially designed Z-Clamps. These accessories are engineered to facilitate secure, fast, and reliable fixing applications.

- Compatible with standard support structures.
- Accessories designed for safe, efficient installation.
- Ensures stability and longevity in demanding environments.

Allmarc can customised planks with any perforation or finishing as per your project requirement.

## Specification of Grip Strut

Customizable dimensions, durable material choices (Mild Steel, Stainless Steel, Aluminum), diverse surface finishes, and standard sizes with 16 diamonds. Its robust monolithic design ensures sturdiness, making it perfect for slip-resistant applications like platforms, walkways, and stair treads in various settings.

Standard Dimension (Customizations on Request):

- Height: 38 / 50 / 75 mm
- Length: Min. 500 mm to Max 8000 mm
- Thickness: 1.6 mm to 2.5 mm

Surface Finish:Self finish, Painting, Pre-Galvanized, Zinc Plating, Powder Coating, Hot Dip Galavanizing

Material of Construction:

Material | Material Grade | Standard Thickness (mm)
--- | --- | ---
Mild Steel | IS 2062: E250 / E 350 | 2.0, 2.5, 3.0, 3.5, 4.0, 5.0
Pre Galvanised | IS 277 | 2.0, 2.5, 3.0, 3.5
Aluminium | As Per Requirement | 2.0, 2.5, 3.0
Stainless Steel | As Per Requirement | 1.6, 2.0, 2.5, 3.0

Allmarc can manufacture planks with any type of custom hooks as per your project requirement.

## Comparison of Conventional Bar Grating & Chequered Plates with Grip Strut

Grip Strut outperforms conventional bar gratings and chequered plates with its lightweight design and superior slip resistance. Its anti-skid surface enhances safety while allowing better drainage, making it ideal for load-bearing applications in industrial and construction settings.

Specification | Chequered Plate | Serrated Bar Grating | Diamond Grip Strut
--- | --- | --- | ---
Sample Dimension | 1000 mm X 500 mm | 1000 mm X 500 mm | 1000 mm X 500 mm
Load Bearing Area | 0.500 Sqm. | 0.500 Sqm. | 0.500 Sqm.
Material | MS-IS:2062 | MS-IS:2062 | MS-IS:2062
Sample Weight (Kg) | ~ 24 Kg | ~ 24 Kg | ~ 13 Kg
Specification | 6 mm Thick Chequered Plate (With 60×6mm Stiffeners @ 700mm C/C) | Flat 25X6 Main Members (@ 35mm C/C + 12mm Dia. ISRO Sec Member @ 75mm c/c) | 3 mm Thick Cold-Stamped (8 pressed Plate with 50mm Side + 10mm Bottom Bends)
Construction Type | Flat Plate with Stiffeners welded underneath | Electroforged (Rod welded over Serrated Flats) | Single Plank / Monolithic design - No welded Joints
Opening / Void | No opening | 35mmX75mm | 15mm x 45mm
Fixing Type / Method | Welding | Clamping | Welding, Bolting, Clamping
Weight / Sqm. | ~48 Kg | ~48 Kg | ~26 kg
Slip Angle / Grade | ~200 to 260/ R-11 | ~INR 1560 (@ -INR65 / Kg) | ~460 / R-13
Uphill Slip Rate @ 100 | Dry Surface = 0% Wet Surface, (Oil) = 8% | Dry Surface = 0% Wet Surface, (Oil) = 0% | Dry Surface = 0% Wet Surface, (Oil) = 0%
Downhill Slip Rate @ 100 | Dry Surface = 0% Wet Surface, (Oil) = 0% | Dry Surface = 0% Wet Surface, (Oil) = 0% | Dry Surface = 0% Wet Surface, (Oil) = 0%
Uphill Slip Rate @ 200 | Dry Surface = 8% Wet Surface, (Oil) = 67% | Dry Surface = 8% Wet Surface, (Oil) = 67% | Dry Surface = 8% Wet Surface, (Oil) = 0%
Downhill Slip Rate @ 200 | Dry Surface = 17% Wet Surface, (Oil) = 83% | Dry Surface = 0% Wet Surface, (Oil) = 58% | Dry Surface = 0% Wet Surface, (Oil) = 8%
Co-efficient of Friction, C.O.F | OSHA Rqmt. = 0.5 | OSHA Rqmt. = 0.5 | OSHA Rqmt. = 0.5

## Looking for Customised Solutionsfor your Project?

Allmarc team will be happy to help you find the ideal solutions tailored to your business or project requirement.
Submit Inquiry Call our Specialist
Inquiry
Whatsapp
Call
Send Inquiry for
Get assured response within 24 hours.

Full name
Company name
Phone
Email ID
Your Message
Your message has been sent successfully!