You are using Internet Explorer and will not be able to use our website properly.
Please change to an up-to-date browser for ideal presentation of the website.

x

# Toe Guard

Designed to enhance safety by preventing the fall of objects and personnel in high-risk areas, toe guards are a crucial element for workplace safety on scaffolding.

## Toe Guard for Elevated Work Zones

Whether for standard or adjustable configurations, we offer stable and cost-effective toe guard solutions tailored to your scaffold setup. Standard specifications for quick reference:

- Fixed Toe Board Length: 1000-3000 mm
- Telescopic Toe Board Length: 1000-1500 mm; 1500-3000 mm
- Standard Heights: 150 mm, 175 mm, 200 mm
- Sheet Thickness: 1.6 mm, 1.8 mm, 2.0 mm
- Material: Mild Steel IS 2062 : E250, Pre Galvanised IS 277
- Surface Finish: Painted, Zinc Coated, Hot Dip Galvanised

3D Representation of Allmarc Toe Guards

## Key Features of Allmarc Toe Guards

Allmarc Toe Guards ensure safety on scaffolding with durable, customizable options.

- #### Fixed Length Toe Board

  - Cost-effective for fixed scaffold sizes.
  - Stable and reliable safety barrier.

- #### Telescopic Toe Board

  - Adjustable for varying scaffold lengths.
  - Quick adaptability and secure fit.

- #### Material & Surface Finish

  - Mild Steel IS 2062 E250, Pre-Galvanised IS 277.
  - Painted, Zinc Coated, or Hot Dip Galvanised.

Actual images of our toe guards at Allmarc factory

## Looking for Customised Solutionsfor your Project?

Allmarc team will be happy to help you find the ideal solutions tailored to your business or project requirement.
Submit Inquiry Call our Specialist
Inquiry
Whatsapp
Call
Send Inquiry for
Get assured response within 24 hours.

Full name
Company name
Phone
Email ID
Your Message
Your message has been sent successfully!