You are using Internet Explorer and will not be able to use our website properly.
Please change to an up-to-date browser for ideal presentation of the website.

x

# Allshore Shoring System

Heavy-duty and reliable, 10 MT load capacity for heavyweight construction, upto 65 mm pipe diameter for stability, and a streamlined spring locking system for efficient, safe assembly.

## Overview of Allshore Shoring System

The Allshore Shoring System is a robust solution engineered for heavy-duty load-bearing in large construction projects. Its high load capacity and durable design make it ideal for infrastructure, industrial, and other large-scale applications. The system ensures maximum stability and safety, supporting loads of up to 10MT with precision and ease.

- Supports high loads with maximum stability
- Modular design for flexible configurations
- Compatible with multiple accessories for easy adjustments
- Designed for quick setup and dismantling

3D Representation of Allshore Shoring System

## Key Features of Allshore Shoring System

The Allshore Shoring System is engineered for high-performance load-bearing and stability, making it ideal for large-scale construction projects.

- #### High Load Capacity

  - Supports up to 10MT of load, ensuring durability in heavy-duty applications.
  - Ideal for infrastructure and industrial projects with high load demands.

- #### Larger Vertical Diameters

  - Increased pipe diameters provide enhanced strength and stability.
  - Perfect for high-rise and large-scale construction requirements.

- #### Modular Design

  - Allows for flexible configurations based on project needs.
  - Easy integration with other construction systems and accessories.

- #### Durable Materials

  - Manufactured from high-strength steel for reliable, long-term use.
  - Resistant to harsh construction environments.

- #### Quick Setup and Dismantling

  - Streamlined assembly process for efficient construction timelines.
  - Easy to dismantle and transport between sites.

- #### Enhanced Safety

  - Designed with built-in safety features to secure operations under heavy load.
  - Prevents slippage and maintains stability throughout the project.

3D walkthrough of how Verticals, Ledgers and Braces are attached with each other.

## Verticals for Allshore Shoring System

The Verticals in the Allshore Shoring System are essential load-bearing members, designed for high strength and durability. They are crafted from top-grade YST 310 steel and feature precision-engineered components for maximum efficiency in heavy-duty applications.

- Steel Type:

  - YST 310 Steel (60% stronger than YST 210)
  - Higher load-bearing capacity for demanding projects

- Rosset Plates:

  - Welded at 500 mm intervals
  - Laser-cut for precision
  - Robotic welding ensures consistency and dimensional accuracy

- Sectional Properties:

  - Diameter: 65 mm
  - Thickness: 3.2 mm
  - Sectional Area: 6.21 cm²
  - Moment of Inertia: 29.74 cm⁴
  - Section Modulus: 9.15 cm³

Actual Images of Verticals for Allshore Shoring System at Allmarc Factory
3D walkthrough of Verticals in Allshore Shoring System

## Specification of Verticals for Allshore Shoring System

Our vertical components are designed with precision to support diverse construction needs while ensuring safety and efficiency on-site.

Part Code | Component | Pipe Dia. x Thick, mm | Length, mm | No. of Rings
--- | --- | --- | --- | ---
ASV-1000 | Vertical | 65 x 3.2 | 1000 | 2
ASV-1500 | Vertical | 65 x 3.2 | 1500 | 3
ASV-2000 | Vertical | 65 x 3.2 | 2000 | 4
ASV-2500 | Vertical | 65 x 3.2 | 2500 | 5
ASV-3000 | Vertical | 65 x 3.2 | 3000 | 6

## Ledgers for Allshore Shoring System

Ledgers are vital horizontal components in shoring systems, designed to support horizontal and lateral loads from planks and walkways. With crimped pipes, investment-cast end connectors, and secure attachment via Rosset plates, Ledgers feature a built-in locking mechanism for stable diagonal bracing.

- Material Properties

  - Steel Grade: YST 310 (60% stronger than YST 210)

- Sectional Properties

  - Sectional Area: 4.53 cm²
  - Moment of Inertia: 11.59 cm⁴
  - Section Modulus: 4.8 cm³
  - Diameter: 48.3 mm
  - Thickness: 3.2 mm

- Design Features

  - End Connectors: Investment casted for maximum strength
  - Rosset Plate Connection: Ensures secure attachment to vertical members
  - Locking Mechanism: Facilitates secure bracing connections

Actual images of Ledgers for Allshore Shoring System at Allmarc Factory
3D Walkthrough of Ledger in Allshore Shoring System

## Specification of Ledgers for Allshore Shoring System

Our ledger components are meticulously engineered to support various construction applications while ensuring safety and efficiency on-site.

Part Code | Component | Pipe Dia. x Thick, mm | Length, mm | Point Load, (W), kN | Two Point Loads, (P+P), kN | Total Load, kN (UDL, kN/m)
--- | --- | --- | --- | --- | --- | ---
ASL-1200 | Ledger | 48.3 x 3.2 | 1200 | 1.95 | 2.50 | 3.42 (2.85)
ASL-1500 | Ledger | 48.3 x 3.2 | 1500 | 1.38 | 1.62 | 2.21 (1.47)
ASL-1800 | Ledger | 48.3 x 3.2 | 1800 | 0.97 | 1.13 | 1.53 (0.85)
ASL-2400 | Ledger | 48.3 x 3.2 | 2400 | 0.71 | 0.87 | 1.13 (0.47)
ASL-3000 | Ledger | 48.3 x 3.2 | 3000 | 0.57 | 0.69 | 0.90 (0.30)

## Braces for Allshore Shoring System

Bracings are diagonal members in the shoring system designed to take inclined loads, transmitting forces directly along their axes. They ensure maximum structural stability and safety in various construction applications.

- Material Properties:

  - Steel Grade: YST 310 (approximately 60% stronger than YST 210)

- Locking Mechanism:

  - Bracings are pressed into the slots in the ledgers for enhanced strength. A pin is then inserted to lock them securely in place.

- Sectional Properties:

  - Diameter: 42.4 mm
  - Thickness: 3.2 mm
  - Sectional Area: 3.94 cm²
  - Moment of Inertia: 7.61 cm⁴
  - Section Modulus: 3.58 cm³

Actual images of Braces for Allshore Shoring System at Allmarc Factory
3D Walkthrough of Braces for Allshore Shoring System

## Specification of Braces for Allshore Shoring System

Our bracing components are meticulously engineered to support various construction applications while ensuring safety and efficiency on-site.

Part Code | Component | Pipe Dia. x Thick, mm | Length, mm
--- | --- | --- | ---
ASB-1200 | Bracing | 48.3 x 3.2 | 1000
ASB-1500 | Bracing | 48.3 x 3.2 | 1500
ASB-1800 | Bracing | 48.3 x 3.2 | 2000
ASB-2400 | Bracing | 48.3 x 3.2 | 2500

## Looking for Customised Solutionsfor your Project?

Allmarc team will be happy to help you find the ideal solutions tailored to your business or project requirement.
Submit Inquiry Call our Specialist
Inquiry
Whatsapp
Call
Send Inquiry for
Get assured response within 24 hours.

Full name
Company name
Phone
Email ID
Your Message
Your message has been sent successfully!