You are using Internet Explorer and will not be able to use our website properly.
Please change to an up-to-date browser for ideal presentation of the website.

x

# Heavy-duty Planks

Allmarc’s custom planks are lightweight, durable, and designed for maximum safety, providing optimal support for modular scaffolding systems worldwide.

## Scaffolding Planks

Allmarc's scaffolding planks are engineered for superior performance, combining slip-resistant surfaces with durability. Ideal for construction projects, our planks are customizable to meet your specific needs. Standard specifications for quick reference:

- Height: 25 mm to 100 mm
- Length: 200 mm to 8000 mm
- Thickness: 1.8 mm to 5 mm
- Width: 200 mm to 1000 mm
- Material: Mild Steel IS 2062 : E250, Pre Galvanised IS 277
- Surface Finish: Painted, Pre Galvanised, Hot Dip Galvanised, Powder Coated

3D Representation of Allmarc Planks

## Key features of Allmarc Planks

Allmarc Planks deliver unmatched traction, durability, and customizable options to suit diverse scaffolding needs.

- #### Slip-Resistant Traction

  - Slip-resistant surface ensures superior grip.
  - Stable for heavy-duty scaffolding in wet conditions.

- #### Perforated for Functionality

  - Circular perforations enable efficient drainage.
  - Lightweight design with enhanced grip.

- #### Durable, Low-Maintenance

  - Constructed from high-strength steel for long-term use.
  - Easy to clean and maintain.

- #### Custom Size Options

  - Available heights: 25 mm to 100 mm.
  - Lengths range from 200 mm to 8000 mm.
  - Widths: 200 mm to 1000 mm, adaptable to various setups.

- #### Material & Finish Choices

  - Materials: Mild Steel IS 2062 E250, Pre-Galvanised IS 277.
  - Finishes: Painted, Pre-Galvanised, Hot Dip Galvanised, Powder Coated.

- #### Built for Heavy Loads

  - Engineered for repetitive use under harsh conditions.
  - Precision fit for seamless scaffolding integration.

Actual images of our planks at Allmarc factory

## Tailored Finishing & Perforations in Planks

Allmarc provides a range of customizable perforations to meet your specific scaffolding needs. From enhanced traction to sleek aesthetics, we design planks that prioritize both function and durability.

- Customised Perforation: Round Dimple, Cross Capsule, Star Capsule, etc.
- Enhanced Safety: Anti-slip surfaces ideal for scaffolding walkways.
- Durability: Robust perforation ensures long-lasting performance.

Allmarc can customised planks with any perforation or finishing as per your project requirement.

## Custom Planks with Versatile Hook Designs

Allmarc's custom planks come with a range of hook options, including raised, forged fix, dog ear, and heavy-duty hooks, offering maximum flexibility and safety in scaffolding systems.

- American Plank Raised Hook for enhanced stability.
- Forged Fix Hook for extra strength and reliability.
- Dog Ear Hook for easy attachment and secure locking.
- Heavy Duty Fix Hook for high-load applications.

Allmarc can manufacture planks with any type of custom hooks as per your project requirement.

## Customised Planks for Every Project

We craft planks precisely tailored to your project’s specifications, ensuring optimal performance and fit.

- Advanced fabrication with cutting-edge technology
- Custom sizes, perforations, and finishes available
- Durable materials to meet any environmental challenge
- Fast and efficient production for timely delivery

Robotic welding in action for joining of plank components at Allmarc factory

## Looking for Customised Solutionsfor your Project?

Allmarc team will be happy to help you find the ideal solutions tailored to your business or project requirement.
Submit Inquiry Call our Specialist
Inquiry
Whatsapp
Call
Send Inquiry for
Get assured response within 24 hours.

Full name
Company name
Phone
Email ID
Your Message
Your message has been sent successfully!